# sustainable Transport: Prescripitve pathway

### Credit 17b

### Design Review Submission As Built Submission

|  |  |  |  |
| --- | --- | --- | --- |
| Total Points available: | 7 | Points claimed: | [#] |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Criteria | Points Available | Points Claimed |
| **17B.1** | **Access by Public Transport** | 4 | [#] |
| **17B.2** | **Low Emission Vehicle Infrastructure** | 1 |  |
| **17B.3** | **Active Transport Facilities** | 1 |  |
| **17B.4** | **Walkable Neighbourhood** | 1 |  |
|  | **TOTAL** | 7 | [#] |

## Project-specific technical questions (formerly tcs and cirs)

|  |  |
| --- | --- |
| There are no project-specific Technical Questions for this credit. |  |
| There are project-specific Technical Questions for this credit and all responses received from the NZGBC are attached. |  |

|  |  |
| --- | --- |
| **Summary of Expected Fitout Occupant Numbers** | |
|  | **Expected Numbers** |
| Regular Occupants | [#] |
| Visitors | [#] |
| Peak Occupancy (Tertiary Education only) | [#] |
| [Other occupant type] | [#] |

### General Information

Provide a description of how the project team has determined these numbers. This justification might make reference to the owner’s project requirements document or similar.

### 17B.1 Access by Public Transport

|  |  |
| --- | --- |
| 17B.1A Projects located within the following postcodes will automatically be awarded 4 points:   * Auckland CBD, postcodes 1010 and 1052 * Hamilton CBD 3204 * Wellington CBD 6011 * Christchurch CBD 8011, 8013\* (\*projects located on or south of Bealey Ave only) * Dunedin CBD 9016 |  |
| 17B.1B Percentage achieved for the project as calculated by the Access Public Transport Calculator | [#] |
| Points being claimed | [#] |

Identify where this information can be found within the supporting documentation provided.

|  |  |
| --- | --- |
| **Supporting Documentation** (Name / title / description of document) | **Reference** (Page no. or section) |
| Access by Public Transport Calculator results | [####] |

### 17B.2 Low Emission Vehicle Infrastructure

Select one of the below compliance methods:

|  |  |
| --- | --- |
| 17B.2A.1 15% of parking is designated for fuel efficient vehicles. |  |
| 17B.2A.2 5% of total parking provided is designated for use by electric vehicles and charging infrastructure is provided. |  |
| 17B.2A.3 Dedicated car share spaces and vehicles are provided at a rate of 1 per 70 occupants (for residential projects only). |  |
| 17B.2B No parking spaces are being provided, and the ‘Low Emission Vehicle Infrastructure’ criterion is made ‘Not Applicable’. |  |

Provide a description of how the project meets the requirements for low emission vehicle infrastructure.

Identify where this information can be found within the supporting documentation provided.

|  |  |
| --- | --- |
| **Supporting Documentation** (Name / title / description of document) | **Reference** (Page no. or section) |
| [####] | [####] |
| [####] | [####] |

### 17B.3 Active Transport Facilities

|  |  |
| --- | --- |
| 17B.3.1 Bicycle parking and associated facilities have been provided for regular fitout occupants. |  |
| 17B.3.2 Bicycle parking has been provided for fitout visitors. |  |

Provide a description of secure bicycle parking spaces and end-of-trip facilities provided.

**Summary of Cycle Facilities**

|  |  |  |  |
| --- | --- | --- | --- |
| **Cycle Spaces for Regular Occupants** | | | |
| Spaces required: | [#] | Spaces provided: | [#] |
| **Cycle Spaces for Visitor** | | | |
| Spaces required: | [#] | Spaces provided: | [#] |
| **End-of-Trip Facilities for Regular Occupants** | | | |
| Facilities required: | [#] | Facilities provided: | [#] |

Identify where this information can be found within the supporting documentation provided.

|  |  |
| --- | --- |
| **Supporting Documentation** (Name / title / description of document) | **Reference** (Page no. or section) |
| [####] | [####] |
| [####] | [####] |

### 17B.4 walkable neighbourhoods

Select one of the below compliance methods:

|  |  |
| --- | --- |
| 17.4A At least four amenities (for industrial facilities) or at least eight amenities (for all other types of buildings) are within 400m of the project. |  |
| 17.4B The project achieves the following Walk Score: | [#] |

Identify where this information can be found within the supporting documentation provided.

|  |  |
| --- | --- |
| **Supporting Documentation** (Name / title / description of document) | **Reference** (Page no. or section) |
| [####] | [####] |
| [####] | [####] |

## DISCUSSION

Outline any issues you would like to highlight and clarify with the Assessment Panel.

## DECLARATION

I confirm that the information provided in this document is truthful and accurate at the time of completion.

Provide author details, including name, position and email address:

[Date]

––– **Report end** –––